**Sample Asbestos-Containing Material List**

|  |  |
| --- | --- |
| • Acoustical ceiling texture(“popcorn”)• Asphalt flooring• Base flashing• Blown-in insulation• Boiler/tank insulation• Breaching insulation• Brick mortar• Built-up roofing• Caulking/putties• Ceiling tiles/panels/mastic• Cement board/transite• Cement pipes• Cement roofing shingles• Chalkboards• Construction mastics• Duct tape/paper• Ductwork flexible connections• Electrical cloth• Electrical panel partitions• Electrical wiring insulation• Elevator brake shoes• Erkot roofing material• Fire blankets• Fire curtains/hose• Fire doors• Fireproofing• Furnace insulation | • Gray roofing paint• High temperature gaskets• HVAC duct insulation• Incandescent light fixture backing• Joint compound/wallboard• Laboratory hoods/table tops• Laboratory fume hood• Mudded pipe elbow insulation• Nicolet (white) roofing paper• Packing materials• Paper fire box in walls• Paper on backside of fiberglassinsulation• Pipe insulation/fittings• Plaster/wall joints• Poured flooring• Rolled roofing• Roofing shingles• Sink insulation• Spray-applied insulation• Stucco• Sub flooring slip sheet• Textured paints/coatings• Vapor barrier• Vinyl floor tile/mastic• Vinyl sheet flooring/mastic• Vinyl wall coverings• Window glazing |

**Note:** *This list does not include every product that may contain asbestos. It is*

*intended as a general guide to show which types of materials may contain*

*asbestos.*